2.72
- fix problem with hardware settings (only for RTC version)

2.71
- add reset settings over "reset.cfg" file

2.70
- device now works more than 24 hours
- improve RTC functionality (only for RTC version)

2.69
- now can be Draw Settings setted to full draw size

2.68
- improve RTC functionality (only for RTC version)
- dip switch now set correct file for autoplay (for DIP switch/LITE)
- now is autoplay plays after any other mode was used

2.67
- draw settings configuration is naw allowed for all version (over ArtNET Guru app)

2.66
- add crash logger
- plays shows longer than 15 minute
- fix autoplay in DIP SWITCH version
- fix switch Autoplay to ArtNET mode

2.65
- correct indication DMX IN for non display moncha
- fix autoplay in DIP SWITCH version

2.64
- Update ArtNET universe filter
- Add showing packets per second of ArtNET stream (only for versions with display)

2.63
- BlackOut over DMX and ArtNET
- Add Play all to Dip switch and Lite/GO version
- Fix Play all function
- Fix LED and display indicators
- Turn off scanners when Brightness is 0
- Interlock/External Ilda - generating DMX out
- Display and control invert
- ArtNET GURU animation preview generator

2.61
-Fixed key lock and autoplay draw image.

2.59
-DMX shift works for Interlock and External ILDA too.

2.56
-Added IP mask to commands 130 and 131.

2.53
-Possibility to change DMX address over searcher broadcast.

2.52
-Fixed serial number read for new searcher.

2.51
-Possibility to change DMX channels order. Added DMX channels strobe,
visible points, fine size X/Y.
-If prod.cfg is in the root, the bootldr.cfg is not deleted - used
for production.

2.0.27
-Sensor menu hidden when no sensors configured.

2.0.26
-Reset support for new displays.

2.0.25
-Master/slave for Fiesta.NET.

2.0.24
-Autoplay and config memory parts merged.
-Possibility to get/set flash memory parts over Ethernet Config.

2.0.23
-Added new server socket to be able to control device settings independent
from Ethernet mode (Ethernet controls).
-Fixed display safe card.

2.0.22
-Fixed brightness map full power point at the left bottom.

2.0.20
-Fixed shutter - it's off now when there's no frame selected over DMX
or in autoplay.

2.0.19
-Possibility to change draw settings over Ethernet. Added draw settings
to Display and box version too.

2.0.18
-OEM version repeat enabled by default.
-Added info screen, when Scan/Input changed in SafeCardMenu.

2.0.17
-Ethernet menu to be able to invert axes, set laser settings and
RGB intensities.
-Fixed slow down menu, when card with no files is inserted.
-Correct redraw of DMX menu, when Ethernet is disconnected.

2.0.16
-New fatfs used - faster SD-card read, faster SD initialization, 
faster 255-frames animations playing.

2.0.15
-Play all function in menu.
-Card commands: set/display/hide hours.
-Fixed clock setting over Ethernet/card.

2.0.14
-Reset the settings with left + right button hold at start.
-Display test is disabled when leaving main menu.
-Added Advanced menu with more options.

2.0.13
-Display test now contains more pictures and Draw Settings can
be changed while some test picture is displayed.

2.0.12
-Laser settings menu for external ILDA.
-Laser settings menu for DMX in.

2.0.11
-Invert settings for Kvant's safe card.

2.0.10
-Laser settings for analog pot.

2.09
-Fixed occassional hang when drawing over Ethernet.

2.07
-Fixed DMX fluent draw (was refreshing display all the time).

2.06
-For Box version if key or external ILDA is used, displays not supported.
